Home | Grain Storage Solutions | Company Profile | Employees | Additional Products | Manuals & Drawings | Brochures | Contact
Non-Stiffened Bins/Silos Stiffened Bins/Silos Hopper Bottom Bins/Silos Aeration & Drying Systems Complete Storage Systems Engineering & Design Models & Specifications | AERATION & DRYING SYSTEMS Proper aeration is an important part of every grain storage system and is essential to maintaining grain quality. Properly operated aeration systems help control insect infestation and moisture migration, reducing grain spoilage and saving money. SCAFCO’s aeration systems can be installed in new or existing storage facilities. We use rigid corrugated, perforated aeration duct made from heavy gauge galvanized steel combined with high efficiency axial aeration fans.
HOPPER BOTTOM BIN AERATION SCAFCO uses rigid perforated and corrugated galvanized steel pipe for aeration in hopper bottom bins. Fans mount below the hopper directing air into internal ducts and up through the grain mass. FLUSH FLOOR AERATION Our Flush Floor systems are easy to install. No pre-forming is required –simply set our formed steel concrete forms in place and pour the floor! Our system includes 14% perforated planks with round perforation holes to minimize clogging. | PERFORATED PLANK FLOOR FOR GRAIN DRYING, FAST ERECTION, EASY CLEANING SCAFCO perforated plank floors ensure fast structure erection, uniform grain drying and easy cleaning. Our interlocking planks are precision roll-formed with 14% perforation and a slight crown for added strength. Planks are supported by heavy-duty legs. Floor design features a complete assembly kit to ensure easy installation.