Home | Grain Storage Solutions | Company Profile | Employees | Additional Products | Manuals & Drawings | Brochures | Contact
Non-Stiffened Bins/Silos Stiffened Bins/Silos Hopper Bottom Bins/Silos Aeration & Drying Systems Complete Storage Systems Engineering & Design Models & Specifications | BUCKET ELEVATORS You can move grain and commodity products at rates up to 40 000 bushels per hour, and to heights up to 200 feet (61 m) with our standard belt and bucket elevators. They feature non-impact style head sections to reduce grain damage during discharge, plus watertight and airtight leg sections. CONVEYING EQUIPMENT SCAFCO’s conveyor systems are designed to move high volumes of material in limited space. Materials travel as a solid mass, eliminating turbulence. The smooth-riding chain with UHMW flight attachments maximizes trough transporting capacity. Our conveying systems can be used for distributing material overhead to bins for loading or unloading, or to an elevator leg for load-out or redistribution. Designed for easy assembly, SCAFCO’s conveyors are also weather-and dust-tight to reduce maintenance costs. GRAIN CLEANING Our rubble separators and grain cleaners can handle all types of grain and maize – even when there is a high moisture and impurity content. Our grain cleaning equipment is totally enclosed and dust-proof, and requires minimal supervision and maintenance. The adjustable aspiration system draws all light particles such as chaff, shells and dust from the free-falling grain across the full width of the machine. Coarse impurities are deposited into the expansion chamber and discharged by a screw conveyor. | BULK WEIGHING Each bulk weighing system design undergoes a detailed application analysis to ensure that the system performs to the highest level of expectations. Optional equipment includes service platforms, test weights, auto lift systems, control gates, power units, in-line voltage regulators and more. GRAIN DRYING SCAFCO offers a wide variety of fan and heater styles. Whether you are natural air-drying or heat-drying grain we will help you select the most appropriate equipment for your application. Our selection includes vane axial and centrifugal fans, multiple fuel heaters, thermostat controls, and more. Effective floor designs for aeration grain spreaders and augers are also engineered to maximize your grain drying system. From hardy grains to delicate drying applications, SCAFCO knows how to handle your drying needs. BAGGING/WEIGHING SYSTEMS These bagging scales are designed to handle a wide variety of different products and the feeders and options vary according to your application’s requirements. These systems are typically accurate within + 3 ounces for a 50-pound bag. They include two-speed belt feeders for full and slow-feed filling, a two-position gravity gate for handling free flowing products such as fertilizers, seeds, pellets and more. Bagging/weighing systems also utilize timer-relay logic to control all scale functions.