Home | Grain Storage Solutions | Company Profile | Employees | Additional Products | Manuals & Drawings | Brochures | Contact
Non-Stiffened Bins/Silos Stiffened Bins/Silos Hopper Bottom Bins/Silos Aeration & Drying Systems Complete Storage Systems Engineering & Design Models & Specifications | CENTRIFUGAL FANS SCAFCO provides a complete range of 50 and 60 Hz, high and low speed centrifugal fans. With over 100 models of fans, there is sure to be one that is right for your application. SCAFCO centrifugal fan housings are precision fabricated from heavy guage galvanized steel which is rust resistant, provides an attractive finish and has a long life. Fan housings are bolted together, using as few pieces as possible to increase the strength and reduce the number of seams that can cause air leakage or wear problems. The fan wheels are specifically designed for superior efficiency and low sound levels. All fan parts including fan wheels, inlet cones and fan housings are matched for optimum efficiency.
Debri/Safey screen offers protection from small particles, and can be removed without disturbing any other parts. | AXIAL FANS SCAFCO axial fans deliver high capacity airflow at maximum performance. Fans feature all-galvanized steel bodies, heavy-duty cast aluminum blades and energy-efficient electric motors. Available in a variety of fan diameters and horsepower ratings.
Easily adjusted leveling feet provide for proper mounting.
Complete aerations systems and transitions that work pefect with SCAFCO fans.
Powered by fully enclosed, high quality, single or three phase motors.
Backwardly inclined airfoil wheels that are designed for superior effeciency and low sound levels.